1. Remove any bur from the Handpiece while in the surgery

2. Prepare the handpieces **first** so you can give them time to drain

3. Remove any visible debris using running water and a soft brush

4. Take the can of oil and select the correct nozzle

5. Shake the can

6. Place the can on a flat surface

7. Place a tissue over the end of the Handpiece

8. Give a half second burst of oil - enough so you hear the bearings go round

9. Check the tissue, if it is clean go to step 11

10. If the tissue is dirty, get a clean part of tissue & repeat step 8 & 9

11. When the tissue is clean, stand the Handpiece, head up, to allow oil to drain ***while*** you reprocess the rest of the instruments.

